Protel Design System Design Rule Check
PCB File : C:\share_archlinux\LED_DISP_ON_SHIFT_RESISTERS\PCB1.PcbDoc
Date     : 9/29/2015
Time     : 11:16:01 PM

Processing Rule : Room 10 (Bounding Region = (212.675mm, 48.856mm, 225.807mm, 69.176mm) (InComponentClass('10'))
Rule Violations :0

Processing Rule : Room 9 (Bounding Region = (199.721mm, 48.856mm, 212.853mm, 69.176mm) (InComponentClass('9'))
Rule Violations :0

Processing Rule : Room 8 (Bounding Region = (186.767mm, 48.856mm, 199.899mm, 69.176mm) (InComponentClass('8'))
Rule Violations :0

Processing Rule : Room 7 (Bounding Region = (173.813mm, 48.856mm, 186.945mm, 69.176mm) (InComponentClass('7'))
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.127mm) (All),(All)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.2mm) (Max=0.508mm) (Preferred=0.254mm) (All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All)
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
Rule Violations :0

Processing Rule : Un-Routed Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=0.025mm) (Max=3.5mm) (All)
Rule Violations :0

Processing Rule : Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All)
Rule Violations :0

Processing Rule : Hole To Hole Clearance (Gap=0.254mm) (All),(All)
Rule Violations :0

Processing Rule : Minimum Solder Mask Sliver (Gap=0.254mm) (Disabled)(All),(All)
Rule Violations :0

Processing Rule : Silk To Solder Mask (Clearance=0.254mm) (Disabled)(IsPad),(All)
Rule Violations :0

Processing Rule : Silk to Silk (Clearance=0.254mm) (Disabled)(All),(All)
Rule Violations :0

Processing Rule : Net Antennae (Tolerance=0mm) (All)
Rule Violations :0

Processing Rule : Silk primitive without silk layer
Rule Violations :0

Processing Rule : Modified Polygon (Allow modified: No), (Allow shelved: No)
Rule Violations :0

Processing Rule : Room 3 (Bounding Region = (121.997mm, 48.856mm, 135.129mm, 69.176mm) (InComponentClass('3'))
Rule Violations :0

Processing Rule : Room 1 (Bounding Region = (96.089mm, 48.856mm, 109.221mm, 69.176mm) (InComponentClass('1'))
Rule Violations :0

Processing Rule : Room 2 (Bounding Region = (109.043mm, 48.856mm, 122.175mm, 69.176mm) (InComponentClass('2'))
Rule Violations :0

Processing Rule : Room 4 (Bounding Region = (134.951mm, 48.856mm, 148.083mm, 69.176mm) (InComponentClass('4'))
Rule Violations :0

Processing Rule : Room 5 (Bounding Region = (147.905mm, 48.856mm, 161.037mm, 69.176mm) (InComponentClass('5'))
Rule Violations :0

Processing Rule : Room 6 (Bounding Region = (160.859mm, 48.856mm, 173.991mm, 69.176mm) (InComponentClass('6'))
Rule Violations :0


Violations Detected : 0
Time Elapsed        : 00:00:02