Field=Comment~String~Comment~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=LibRef~String~LibRef~100|Field=Quantity~Integer~Quantity~100|Field=Value~String~Value~100|Field=Footprint~String~Footprint~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~AD.PrjPcb|ReportField=ProjectFullPath~C:\share_archlinux\fifth_wheel_speed\AD\AD.PrjPcb|ReportField=Title~Bill of Materials For Project [AD.PrjPcb] (PCB Document : PCB1.PcbDoc)|ReportField=TotalQuantity~55|ReportField=ReportTime~8:32:26 PM|ReportField=ReportDate~11/17/2015|ReportField=ReportDateTime~11/17/2015 8:32:26 PM|ReportField=OutputName~Bill of Materials|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~None|ReportField=Address1~|ReportField=Address2~|ReportField=Address3~|ReportField=Address4~|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~|ReportField=Author~|ReportField=CheckedBy~|ReportField=CompanyName~|ReportField=CurrentDate~11/17/2015|ReportField=CurrentTime~8:21:51 PM|ReportField=Date~|ReportField=DocumentFullPathAndName~C:\share_archlinux\fifth_wheel_speed\AD\Sheet1.SchDoc|ReportField=DocumentName~Sheet1.SchDoc|ReportField=DocumentNumber~|ReportField=DrawnBy~|ReportField=Engineer~|ReportField=ImagePath~|ReportField=ModifiedDate~11/13/2015|ReportField=Organization~|ReportField=ProjectName~AD.PrjPcb|ReportField=Revision~|ReportField=Rule~|ReportField=SheetNumber~|ReportField=SheetTotal~|ReportField=Time~|ReportField=Title~|ReportField=DataSourceFileName~AD.PrjPcb|ReportField=DataSourceFullPath~C:\share_archlinux\fifth_wheel_speed\AD\AD.PrjPcb|ReportField=PCBDataSourceFileName~PCB1.PcbDoc|ReportField=PCBDataSourceFullPath~C:\share_archlinux\fifth_wheel_speed\AD\PCB1.PcbDoc
Res3|Resistor|R3, R4|Res3|2|?R|J1-0603
Res3|Resistor|R7|Res3|1|500R|J1-0603
Res3|Resistor|R8, R9|Res3|2|270R|J1-0603
Res3|Resistor|R1|Res3|1|100R|J1-0603
Cap Semi|Capacitor (Semiconductor SIM Model)|C5, C6|Cap Semi|2|22pF|1608[0603]
Res3|Resistor|R2|Res3|1|10K|J1-0603
Res3|Resistor|R5, R6, R10, R11, R12, R13|Res3|6|1K|J1-0603
Cap Semi|Capacitor (Semiconductor SIM Model)|C3|Cap Semi|1|0.33uF|1608[0603]
Cap Semi|Capacitor (Semiconductor SIM Model)|C1, C2, C4|Cap Semi|3|0.1uF|1608[0603]
16MHz|Crystal Oscillator|Y1|XTAL|1||HC-49U
ATmega168PA-AU|8-bit AVR Microcontroller, 16KB Flash, 512 Bytes EEPROM, 1KB SRAM, 32-pin TQFP, Industrial Grade (-40°C to 85°C)|U1|ATmega168PA-AU|1||32A_N
Header 3|Header, 3-Pin|power_for_5wheel, power_select|Header 3|2||HDR1X3
Header 5X2|Header, 5-Pin, Dual row|P1|Header 5X2|1||HDR2X5
L7805ABD2T-TR|Positive Voltage Regulator, 3-Pin D2PAK, Tape and Reel|U2|L7805ABD2T-TR|1||TO-263_M
out_pad||5wheel_power, but_mode, but_mode_GND, but_resDist, but_resDist_GND, car_+12V, car_GND, data, disp_gnd, disp_vcc, enc_a, enc_b, enc_GND, led_GND, led_green, led_red, pb5, pc2, pc3, pc4, pc5, pd0, pd1, pd7, shcp, stcp, wheel_A, wheel_B, wheel_GND|out_pad|29||pad
speaker||speaker|speaker|1||speaker
